*USED PARTS FOR SALE AT OUR SHOP*

*$400.00*

**5.3 LS block**; This aluminum block had been prepped for rebuild. Standard bore, line bore has been checked, cylinders are standard size and have been honed.

*$1000.00*

**CNC ported LS heads;** 317 castings, full CNC port work, multi angle valve job, new stainless intake and exhaust valves. 2.02 intake valves. 71cc combustion chambers.